Tabulato caratteristiche minime

Lotto 1

**Personal Protective Equipment**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 1** | **Protective helmet** | **C** | **D** |
| **Purpose:** | Multifunctional head protection |  |  |
| **Technical specification** | Highly resistant shell to shocks, exposure to elevated temperatures and chemical attack  Vented shell available to optimize user’s breathability  3- point chinstrap for safe fit. Adjustable in 5 steps, with automatic buckles, flexible chin cup  Height-adjustable headband and net suspension  CE marking: To EC Directive 89/686/on Personal Protective Equipment   * EN16471:2014 – Wildland • fire helmet * EN16473: 2014 – Technical Rescue helmet * EN12492: 2021 – Mountain Climbing   Weight Helmet (without accessories): 650 g +/- 20g Accessories (included)  Helmet mounted LED flashlight Safety Goggles (EN166)  Neck curtains (textile)  Retro-reflective stripes to enhance wearer’s visibility in low light conditions - silver  Colours - 2 red/ 23 yellow  Options - possibility (not included in order)  Helmet mounted hearing protection for noisy applications  Helmet mounted voice communication headsets to enable connection to portable radios  Compatibility with Full face mask |  |  |
| **As an example only** | MSA Gallet F2 X-TREM |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Example** | Immagine che contiene casco, copricapo  Descrizione generata automaticamente |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 2** | **Under helmet protection** | **C** | **D** |
| **Purpose** | Protects forest fire fighters from burns on the face and neck. |  |  |
| **Technical specification** | For use in a situation of risk with high exposure to thermal risk Compatible with respiration equipment and helmets  Weight max 250gr  Made of fire-retardant material - permanently non-flammable textile. EN 13911 – Protective clothing for firefighters  EC mark  One size fits all |  |  |
| **As an example only** | Vallfirest, Comazo |  |  |
| **Example** | C:\Users\doment\Pictures\Pasamontañas%202.jpg Podkapa Comazo - Nomex |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 3** | **Overalls** | **C** | **D** |
| **Purpose** | Heat protection |  |  |
| **Technical specification** | Standards:  - EN 15614: 2007 A1, A2; EN 1149:2008  Material and requirements:   * Light two piece (separate trouser and jacket) single layer clothes. * Made out of flame-resistant meta aramid - fabric, (Nomex) total weigh 220 g/m2 (+-5 %). * Cuff on trousers below. * All reinforcements made of double-layer Nomex or lined. * Colour of reflective strips: yellow – grey – yellow. |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | - Colour: dark blue.  Jacket  The shape of jacket is basic, allows movement in all directions and does not twist or raise in any position. In front part are pockets. At waist height, one pocket on each side covered with a flap and protected with Velcro closure. In pockets are loops equipped with carabiner. Chest pockets on left side for radio station with two fixations for microphone. On right side Lamp holder and two pockets. The shoulders are reinforced with double fabric. The elbows are reinforced with double fabric. The elbow part is ergonomically designed.  Sleeves are comfortly shaped and have tightenings on ends. Back part is prolonged. On the back side in inscription of the fire brigade (separately by Velcro tape). Jacket has a zipper to pair with the trousers.  Trousers  In waist high there are loops to insert belt and suspenders with regulation of length. On sides are two pockets closed with zippers. Also trousers have two large pockets covered with flaps with Velcro closure protection. End of trousers have regulation of width. Down part have prolongated cuffs, dark colour. There is a bauble fabric reinforcement on the knee. The knee part is ergonomically designed. On back part there is one pocket. In the right side is loop for karabiner. Trousers have a zipper to pair with the jacket. | | |  |  |
| **As an example only** | BAS Lovrenc Slovenia, DEVA Bushfire (separate trouser and jacket) | | |  |  |
| **Example** | Deva spredaj | Deva zadaj | Deva hlače |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 4** | **Under overalls** | **C** | **D** |
| **Purpose** |  |  |  |
| **Technical** | Standards: |  |  |
| **specification** | - SIST EN ISO 13688:2013 |  |  |
|  | - SIST EN ISO 11612:2015 |  |  |
|  | - SIST EN ISO 14116:2015 |  |  |
|  | - SIST EN ISO 1149-5:2018 |  |  |
|  | - EN 340 |  |  |
|  | Material and requirements: |  |  |
|  | - Nomex Comfort, fine knitting 50% aramid with antistatic fiber, 50% |  |  |
|  | Viscose FR |  |  |
|  | - Weight min 210 g/m2 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | * Thermal protection * Fire protection | |  |  |
| **As an example only** | FireFighters – FF outlast combat comfort | |  |  |
| **Example** | [http://www.firefighters.eu.com/si/outlast-produkti/320-ff-outlast-combat-](http://www.firefighters.eu.com/si/outlast-produkti/320-ff-outlast-combat-comfort-fitted-t.html) [comfort-fitted-t.html](http://www.firefighters.eu.com/si/outlast-produkti/320-ff-outlast-combat-comfort-fitted-t.html) | |  |  |
| Podobleka majica | Podobleka hlače |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 5** | **Boots** | **C** | **D** |
| **Purpose** | Legs protection and chain saw protection |  |  |
| **Technical specification** | Standards:   * EN15090 – Footwear for firefighters * Category F2A * EN ISO 17249 – Safety footwear with resistance to chain saw cutting chainsaw cut resistant level 1   Material and requirements:   * Height app. 22 cm, * Water-repellent and breathable suede leather app. 2.0-2,7 mm * Gore-Tex Performance Comfort Footwear * Heat resistant at app. 3000C * Slip-resistant sole * Waterproof * Fire resistant * Sunrays mirror system – the leather reflects the sunrays ensuring the foot better comfort * High energy absorption in the heel * High quality leather * Protect of front part resistant to wear and abrasions from external objects |  |  |
| **As an example only** | Jolly Sawyer pro or similar |  |  |
| **Example** | Jolly sawyer pro6515-GA |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 6** | **Duty Belt with carrier for 2 water bottle and equipment** | **C** | **D** |
| **Purpose** | Bearing personal essentials (water, phone, weather station,…) |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Technical specification** | Duty belt  Carrier fo2 2 plastic bottle of water Carrier for small PPE |  |  |
| **As an example only** | 5.11 SKYHAWK 1.5" BELT, |  |  |
| **Example** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 7** | **Gloves** | **C** | **D** |
| **Purpose** | Hand protection |  |  |
| **Technical specification** | Standard:   * DIN EN 659: 2008 (EN 659+A1+AC:2009) – Protective gloves for firefighters * CE marking   Colour:   * black   Materials and requirements:   * Kevlar, Nomex, * Inside hand, backhand & knuckle protection: special leather, heat resistance, water repellent, special softness, cut resistance, teat resistance, puncture resistance, oil and grease resistance, fire resistance, cold resistance, * Internal lining: made of close-meshed knitted material 100% Kevlar, * Cuff: special leather, long cuff, adjustable strap with flap and Velcro closure, * Insert: moisture barrier, waterproof, windproof, breathable, * Accessories on the glove: ring and claps,   - Sizes: 6 – 13,   * Length: app. 37 cm.   Maintenance:   * Easy to clean, * Easy to storage, * Easy to maintenance. |  |  |
| **As an example only** | Asko Patron Fire |  |  |
| **Example** | gamat-asko-patronfire-dolge-black |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 8 e Item 9** | **Headlamp** | **C** | **D** |
| **Purpose** | Personal illumination. |  |  |
| **Technical specification** | Requirements:   * Luminosity: min 150 lumen. * Power source: battery AAA * Weight: under 100g with batteries * Water tightness: IPX4 (weather-resistant) * reserve AAA batteries 4 pcs. |  |  |
| **As an example only** | Petzl Tikkina 250 or equivalent |  |  |
| **Example** | Čelna svetilka Petzl Tikkina 250 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 10** | **T-shirt** | **C** | **D** |
| **Purpose** | Body protection (for wear on station and provide thermal protection) |  |  |
| **Technical specification** | Standard:  - SIST EN ISO 14116: 2008, EN 340, Öeko tex Standard 100  - SIS EN ISO 14116: 3/5H/40  Material: NOMEX or Armadillo Merino Colour: blue  Requirements: Crew neck Comfort fit Easy care |  |  |
| **As an example only** | Short (Long) Sleeve T-Shirt Heathcoat  Valfirest Armadillo Merino® Cougar Big Cat black |  |  |
| **Example** | heatcoat 21001-01-Cougar-Black-F-MR |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 11** | **Face protection** | **C** | **D** |
| **Purpose** | Face and breathing protection |  |  |
| **Technical specification** | Standard:  - EN 15614  - EN 531  Material and requirements: |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | * Breathing zone tissue composition: 64% viscose, 34% aramid, 2% antistatic, * Fabric composition: Lenzing F.R. 65%, Nomex 30%, Kevlar 5% * Grammage: app. 260 g/m2, * Double-layer Nomex, * Weight: app. 120 g, * Double Velcro system for use and rest and can be comfortably worn hanging from the neck when not being used, * It can be put on without having to take the helmet off, * Ergonomically adjustable in the neck and face areas, * Interchangeable cartridge filter.   Maintenance:   * Easy to clean, * Easy to storage, * Easy to maintenance. |  |  |
| **As an example only** | Vallfirest: vtf protective mask |  |  |
| **Example** | Nomex zaščita s filtrom |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 12** | **Face mask** | **C** | **D** |
| **Purpose** | Breathing protection |  |  |
| **Technical specification** | Standard:   * EN 149:2001+A1:2009 – Respiratory protective devices – Filtering half masks to protect against particles – Requirements, testing, marking * FFP 2   Material and requirements:   * The convex shape, twin strap design, nose foam and nose clip * Effective protection against fine particles * Cool Flow Exhalation Valve * Comfortable with vtf protective mask * Provides lightweight comfort and effective respiratory protection against * Recommends with carbon layer. |  |  |
| **As an example only** | 3M Particulate Respirator, FFP2 |  |  |
| **Example** | Respirator |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 13** | **Backpack** | **C** | **D** |
| **Purpose** | Load bearing |  |  |
| **Technical specification** | Requirements:   * Material: Tearproof and impermeable Cordura material * Capacity: min 20l * Dimensions: about 46(h) x 28 x 14 cm * Hydration system compatible * Colour black |  |  |
| **As an example only** | Tasmanian Tiger MODULAR DAYPACK XL, Brandit US Cooper Medium or equivalent |  |  |
| **Example** | Description: https://www.tasmaniantiger.info/en/wp-content/uploads/sites/3/7159040a-1200x1200.jpg |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 14** | **First aid kit** | **C** | **D** |
| **Purpose** | Personal First aid kit |  |  |
| **Technical specification** | Size: app 14 cm x 10,5 cm x 8 cm  Material for bag: Polyester (Nomex optional) Contents:  1 x BANDAGE FOR FIRST AID TYPE 1  1 x FOLDER 5 x 5 cm, 16 fig. - STERILE  1 x FOLDER 5 x 8 cm, 16 fig. - STERILE   1. x VIVAPLAST a ׳ 10 pcs - HANGER 2. x TOSAMAPLAST PATCH 10 x 6 cm   1 x MICROPORE 12.5 mm pos. pak. 1 x SCISSORS   1. x TRIANGULAR ROUTE 2. x VIVALA BANDAGE 8 cm x 4m 3. x SAFETY CLAMP   1 x ABSORBENT GASE 0.4 m2 - STERILE  1 x LIST OF CONTENTS |  |  |
| **As an example only** | Tosama personal First aid kit |  |  |
| **Example** | i |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 15** | **Sun protection hat** | **C** | **D** |
| **Purpose** | Sun protection |  |  |
| **Technical specification** | UV protection: UPF 50+  Material: cotton or cotton like feel: soft, lightweight, breathable, quick dry performance  Wide protective brim Colour: Navy blue or similar  One size approx. 60 cm with adjustable band  Sign of IPA FF at the front size (approx. 4,5\*6 cm) and EU flag (approx. 1,5\*3 cm) |  |  |
| **As an example only** |  |  |  |
| **Example** | C:\Users\doment\Pictures\02521-410-1000-LD1-coolibar-chlorine-resistant-bucket-hat-upf-50.jpg |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 16** | **Hand tool** | **C** | **D** |
| **Purpose** | Personal tool |  |  |
| **Technical specification** | Requirements:   * Tools materials: Stainless Steel * Closed Length: max 12 cm * Weight: max 300 g * Width: 4,5 cm * Overall Thickness: 2,5 cm * Must include following tools:   + Pliers   + Wire Cutters   + Knife   + Serrated Knife   + Saw   + Phillips Screwdriver   + Large Screwdriver   + Small Screwdriver |  |  |
| **As an example only** | Leatherman Bond or equivalent |  |  |
| **Example** | Description: Leatherman Sidekick, Srebna, Večnamensko orodje |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 17** | **Box for PPE** | **C** | **D** |
| **Purpose** | Loadbearing, storage |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Technical specification** | Requirements:   1. Volume: about 89 l or more 2. Internal dimensions: app. 780x410x330 mm 3. External dimensions: app. 807x470x345 mm 4. Material: plastics |  |  |
| **As an example only** | Explorer Case 78 MUB |  |  |
| **Example** | MUB 78 Case | Explorer Cases UK |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 18** | **Sleeping bag** | **C** | **D** |
| **Purpose** |  |  |  |
| **Technical specification** | Insulation: G-LOFT®, 100% Polyester Outer fabric: 100% Polyamide  Inner lining: 100% Polyamide Sizes: M, L  Dimensions (cm): 215/85/60 (M), 230/87/65 (L) Weight (g): 1.050 (M), 1.200 (L)  Pack size compressed: 18x25 (M), 18x28 (L) Comfort Temp. Ratings: 4 C°  Extreme Temp. Ratings: -10 C° |  |  |
| **As an example only** | Carinthia DEFENCE 1 TOP |  |  |
| **Example** | Carinthia Defence 1 Top Military Sleeping Bag – Perunika |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 19** | **Sleeping mat - wide** | **C** | **D** |
| **Purpose** |  |  |  |
| **Technical specification** | Material: EVA Weight: 480 g  Size: 190x60x1,4 cm Thermal resistance: 2,0 |  |  |
| **As an example only** | YATE EVA COMFORT WIDE 1,4 Black Mat + Rubber Bands |  |  |
| **Example** | YATE EVA COMFORT WIDE 1,4 Black  Mat + Rubber Bands |  |  |

Quantity: specified individually **Technical specification**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 20** | **Trailer for team equipment** | **C** | **D** |
| **Purpose** | Storage of team equipment |  |  |
| **Technical specification** | Requirements:   * Stable trailer construction * According to torsion suspension * All metal parts of the chassis and superstructure are protected against corrosion * Front support wheel * Maximum permissible weight 750 kg * Length min 2000 m * Width min 1070 m * Red tarpaulin with frame * The tarpaulin must open from four sides * Anchorages for equipment * The trailer complies with CE regulations * Inertia brake (As an example only)   Team equipment installed in a trailer:   * Backpack fire pump (12 pieces) * Fire swatters (8 pieces) * Blower (8 pieces) * Petrol containers (2 pieces) * Petrol containers for chain saw (4 pieces) * Forestry axe (2 pieces) * Small axe (2 pieces) * Firefighter axe (2 pieces) * Drip torch (2 piece) * Protection trousers for using chainsaw (4 pieces) * Chain saw (4 piece) * Shovels (8 pieces) * Hoes (8 pieces) * Portable pump (1 piece) * Backpack with fuel (for portable pump) (1 piece) * Portable containers for water (1 piece) * Spare parts adapters and accessories (for portable pump) (1 complete) * Pop up tent * Camp table * Camp chair |  |  |
| **As an example only** | Ključavničarstvo Bartolj d.o.o., Euro GV, Webo.Si |  |  |
| **Example** | Immagine che contiene testo, sedile  Descrizione generata automaticamente |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 21** | **Shovel** | **C** | **D** |
| **Purpose** | Trench digging |  |  |
| **Technical specification** | Wooden handle, round tip, high cutting capacity, resistance to wear and tear. |  |  |
| **As an example only** | Vallfirest Forestry service round shovel |  |  |
| **Example** | Slika, ki vsebuje besede lopata, orodje, sekira  Opis je samodejno ustvarjen |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 22** | **Hoe** | **C** | **D** |
| **Purpose** | Digging a fire line |  |  |
| **Technical specification** | Requirements:   * Metal hoe with wooden handle, * Heart shape, * Handle length app. 130 cm, * Weight app. 1 kg * Width of metal part app. 15 cm * The tool must be strong. |  |  |
| **As an example only** | Kovačija Kremelj Slovenia |  |  |
| **Example** | Motika (3) |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 23** | **Chain saw** | **C** | **D** |
| **Purpose** | Cutting firebreaks |  |  |
| **Technical specification** | * Displacement: 45,6 cm3 * Power output: 2,2 kW * Weight: 4,8 kg (without fuel, without bar and chain) * Power to weight ratio: 2,2 kg/kW * Blade: 40 cm   SIST EN ISO 11681-1 |  |  |
| **As an example only** | Stihl MS251 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Example** | C:\Users\HP\AppData\Local\Microsoft\Windows\INetCache\Content.MSO\50FE4D1F.tmp |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 24** | **Protection trousers** | **C** | **D** |
| **Purpose** | Chainsaw protection |  |  |
| **Technical specification** | Standard:   * EN 381 – Protection clothing for users of hand-held chainsaws * EN 381 – 5 – Protection clothing for users hand-held chainsaws Part 5: Requirements for leg protectors   Requirements:   * Saw protection, * Class 1 (20 m/s), * Quick and easy to put on and off, * Made from tough polyester/cotton twill, * Full long zippers on back of leg or clamp buckle of closures for fast fitting and removal, * Waist adjustment with clamp buckle, * Universal size, * Completely covered chainsaw protection pad. The saw protection pad is completely covered to saw dust doesn’t compromise the performance of the fibre layers. * Reinforced protection pad.   Maintenance:   * Easy to clean, * Easy to storage, * Easy to maintenance. |  |  |
| **As an example only** | Husqvarna Classic, Stihl |  |  |
| **Example** | Zaščitne hlačnice Husqvarna https://i.pinimg.com/564x/6e/3e/f8/6e3ef835f67852db2f536d50e80d648b.jpg |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 25** | **Petrol containers for chain saw** | **C** | **D** |
| **Purpose** | Plastic fuel can for gasoline and oil |  |  |
| **Technical specification** | Capacity: 5 litres/2 litres Material: Heavy duty plastic Safety requirements UN/BAM  Comes complete with pouring spout |  |  |
| **As an example only** | Husquvarna, Stihl |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Example** | 0013683_posoda-za-gorivo-in-olje-husqvarna-52l_550 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 26** | **Backpack fire tank (pump)** | **C** | **D** |
| **Purpose** | Extinguishing |  |  |
| **Technical specification** | Requirements:   * Capacity app. 20 l, * Length of hose app. 1 m, * Light weight app. 2,5 kg, * Ergonomic backpack: flexible pump with protected tank, personalized belt and padded straps., * Fast connection system: Quick hose connection/disconnection system. It allows to work from both the right and the left., * High-visibility colour, * Cushioned shoulder and waist cinches, * Attachment strap for the chest, * Double load adjustment on shoulder to balance the centre of gravity and distribute weight over waist and shoulders., * Double-piston lance, continuous stream, app. 8 litre-per-minute performance, mist and stream options, * Multi-Velcro tool and lance-holder system: transport tools and telescopic fire swatters, * Pocket for accessories on the backside. |  |  |
| **As an example only** | Vallfirest backpack fire pump or Ermak 20 |  |  |
| **Example** | Naprtnjača VF (2) Slika, ki vsebuje besede gospodinjski aparat  Opis je samodejno ustvarjen |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 27** | **Fire swatter** | **C** | **D** |
| **Purpose** | Fire suffocation and scraping |  |  |
| **Technical specification** | Light, textile or leather belts Tear-resistant cotton multilayer Weight: 1,6 kg.  Rigid handle material: Aluminium Flexible handle material: Pom C Delrin  Blade composition: Tear-resistant cotton multilayer and self-extinguishing synthetic rubber. |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Shovel work surface: 40 x 25 cm. Folded length: 92 cm.  Unfolded: 2 m |  |  |
| **As an example only** | Valfirest Fire Swatter vft |  |  |
| **Example** | batefuego_ppal-familia |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 28** | **Firefighting - mist blower** | **C** | **D** |
| **Purpose** | Cleaning areas where the deposits can cause a fire |  |  |
| **Technical specification** | * Displacement: 64,8 cm3 * Weight: 10,2 kg (weight excluding fuel, fully assembled) * Blowing force: 32 N (combination of air speed and air throughput) * Air speed with round nozzle: 89 m/s * Max air speed: 106 m/s * Air throughput: 1.150 m3/h (with round nozzle in blower mode) * Max air throughput: 1.720 m3/h (without blower attachment/nozzle) |  |  |
| **As an example only** | Stihl BR600, Cifarelli |  |  |
| **Example** | BR 600 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 29** | **Portable pump – high pressure** | **C** | **D** |
| **Purpose** | Fire extinguishing |  |  |
| **Technical specification** | * 1-stage centrifugal pump and a 4-stroke engine * Displacement min 49 cm3 * Performance of up to 6,9 bar and a maximum flow of up to 260 l/min * Convenient transport (easy transfer in a load-carrying backpack) * Weight appx. 9,5 kg * Made of lightweight aluminium alloy * Includes a built-in clutch for an easy start, that also allows to stop the discharge of water without switching off the engine * Backpack with fuel (for portable pump) * Extension fuel line kit |  |  |
| **As an example only** | Portable fire pump Black Hawk 1 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Example** | Immagine che contiene tagliaerba, casco  Descrizione generata automaticamente  <https://www.vallfirest.com/en/portable-fire-pumps/portable-fire-pump-bh1> |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 30** | **Spare parts adapters and accessories** | **C** | **D** |
| **Purpose** | For portable pump |  |  |
| **Technical specification** | Equipment   * Suction hoses storz C (4 pieces) * Distributor with ball-valves, storz C/DCD (1 piece), D/DD (6 pieces) * Adapters storz (C-D 4 pieces, B-C 2 pieces) * Multi-purpose branch pipe, size D (4 pieces) * Suction strainers, storz C (1 piece) * In-line ball type valves storz C (3 pieces) |  |  |
| **As an example only** | JMW Fire, AWG |  |  |
| **Example** | <https://www.jmw-fire.com/jmw-doo/JMW-fire-doo-Catalogue.pdf> |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 31** | **Drip torch** | **C** | **D** |
| **Purpose** | Flashback protection |  |  |
| **Technical**  **specification** | 5 litre capacity, Check valve |  |  |
| **As an example only** | Vallfirest Drip Torch 5 litres |  |  |
| **Example** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 32** | **Axe heavy** | **C** | **D** |
| **Purpose** | Heavy axe for forester |  |  |
| **Technical specification** | Weight: 1.60kg Handle length: 80cm Handle material: wood |  |  |
| **As an example only** | Forester heavy axe  https://[www.kovastvo-krmelj.si/trgovina/product/show/productID=2](http://www.kovastvo-krmelj.si/trgovina/product/show/productID%3D2) |  |  |
| **Example** | 0101_ca41cf254ab9c97d37540316b36474e5 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 33** | **Axe light** | **C** | **D** |
| **Purpose** | Light axe for forester or home |  |  |
| **Technical specification** | Weight: 0.60kg  Handle length: 38cm Handle material: wood |  |  |
| **As an example only** | https://[www.kovastvo-krmelj.si/trgovina/product/show/productID=13](http://www.kovastvo-krmelj.si/trgovina/product/show/productID%3D13) |  |  |
| **Example** | 0112 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 34** | **Hose storz C 15m** | **C** | **D** |
| **Purpose** | Fire water distribution |  |  |
| **Technical specification** | Storz C adapter, length 15m DIN 14811 |  |  |
| **As an example only** | Parsch TOP SYNTHETIC C and B 15m, Heberkorn Flammenflex G Ultra |  |  |
| **Example** | Immagine che contiene interni  Descrizione generata automaticamente |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 35** | **Hose storz D 15m** | **C** | **D** |
| **Purpose** | Water distribution |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Technical specification** | storz D adapter, length 15m DIN 14811 |  |  |
| **As an example only** | Technolen Pyrotex hose D 25 15m, Heberkorn Flammenflex G Ultra |  |  |
| **Example** | Immagine che contiene elettronico  Descrizione generata automaticamente |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 36 e Item 37** | **keys for storz B,C, D (coupling spanners)** | **C** | **D** |
| **Purpose** | Connection hose (storz) |  |  |
| **Technical specification** | B Ø75 mm C Ø52 mm D Ø25 mm |  |  |
| **As an example only** |  |  |  |
| **Example** | Rosenbauer ključi za spojke - Rosenbauer  Rosenbauer ključi za spojke - Rosenbauer |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 38** | **Portable container** | **C** | **D** |
| **Purpose** | Portable water container - water tender |  |  |
| **Technical specification** | * They are used for creating water supplies for fire extinguishing * Material: polyester fabric coated with NBR/PVC provides resistance to UV rays, ozone and other heavy weather conditions * Storz C system * Inflation hose for inflatable collar (with the connector tot he compressor) * Groundsheet * Packing bag * Hand pump * Capacity: appx. 1000 l |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **As an example only** | Trelleborg Slovenia Savatech |  |  |
| **Example** | [https://www.trelleborgslovenija.com/images/eko/2020/HAZ-](https://www.trelleborgslovenija.com/images/eko/2020/HAZ-MAT_Trelleborg_katalog_2020_ang.pdf) [MAT\_Trelleborg\_katalog\_2020\_ang.pdf](https://www.trelleborgslovenija.com/images/eko/2020/HAZ-MAT_Trelleborg_katalog_2020_ang.pdf) |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 39** | **Indication vest (for mng)** | **C** | **D** |
| **Purpose** | Multifunction vest for incident manager |  |  |
| **Technical specification** | Material: Modacryl cotton or nomex Size: Universal  Colour: Yellow (Gold), Grey (Silver) Details (optional):   * Two microphone holders * Fastening option for name and ID signs on front * Two radio pockets, right pocket with an additional snap hook * Two side pockets * Double front zip with quick-release buckles * Side width adjuster with clamp buckles * Fastening option for two back ID signs * Hook and loop straps for fastening to the coat |  |  |
| **As an example only** | S-GARD Multifunction vest |  |  |
| **Example** | gamat-sgard-brezrokavnik-rumen_1 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 40** | **Large multi-LED hand torch** | **C** | **D** |
| **Purpose** | illumination |  |  |
| **Technical specification** | Requirements:   * min 1500 lumens, * up to 100 hrs burn time, * water and dust resistant - IPX54 min. |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **As an example only** | LEDLENSER P18R Work or equivalent |  |  |
| **Example** | Description: https://www.mall.cz/i/55599411/1000/1000 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 41** | **Weather station** | **C** | **D** |
| **Purpose** | Measuring weather conditions |  |  |
| **Technical specification** | Current wind speed Maximum Wind Gust Average Wind Speed  Air, water & snow temperature Wind chill  Barometric Pressure Altitude  Real-time clock  Protective cover with sure-grip overmoulding Data hold function  Large easy-to-read display with backlight Waterproof and floats  Quick response, external thermistor High precision pressure sensor  Night Vision |  |  |
| **As an example only** | Kestrel 2500 Pocket Wind meter night vision |  |  |
| **Example** | Immagine che contiene testo, dispositivo, calibro  Descrizione generata automaticamente |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 42** | **Backpack selfrescue for reconnaissance** | **C** | **D** |
| **Purpose** | Selrescue backpack with emergency respiration system and extreme shelter |  |  |
| **Technical specification** | Xtreme Pack   * Weight 1.25 kg. * Harness size (S-M) and (L-XL). * Hydration system 2.8 l |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Xtreme Shelter XS 17   * Weight: 1,35 * Dimensions when folded: 39 x 17 x 6 cm * Standard:   - EN ISO 9151:2018  - EN ISO 11612:2018  - EN ISO 6942:2002   * Levels A1, B1, C4. Xtreme K * Weight: 1,5kg * Autonomy: no less than 20 minutes   - Standard: EN 13794:2002 |  |  |
| **As an example only** | Vallfirest Xtreme Kit |  |  |
| **Example** | xtreme-kitok |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 43** | **Backpack for carrying equipment** | **C** | **D** |
| **Purpose** | loadbearing |  |  |
| **Technical specification** | Requirements:   * size adjustment system (height) * padded belt with reinforcement * aluminium frame |  |  |
| **As an example only** | vft hose carrying backpack (vallfirest shop) or equivalent |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Example** | Description: https://www.vallfirest.com/media/products/229/521-1951.jpg |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 44** | **First aid backpack** | **C** | **D** |
| **Purpose** | First aid equipment for team member |  |  |
| **Technical specification** | Material of backpack: Polyester Size: min. 27×20×47cm Colour: red  or:  Dimensions: about 48x29x60(h) cm Weight: about 2,5 kg  Material: Tear proof and impermeable Cordura material Specifications:  4 refractive strips  8 removable coloured pouches 3 perimetric external pouches  Independent and removable mini-rucksack frontally placed through zipper  CONTENTS OF THE PERSONAL KIT BAG FOR PP  2 pieces Compress ALU layer for burns 50 x 60 cm, sterile  5 pcs Compress ALU layer 5 x 9 cm, individually packed, sterile   1. pieces Compress ALU layer 15 x 9 cm, individually packed, sterile 2 pcs Bandage, first sterile - TYPE I 2. pcs Bandage, first sterile - TYPE II 2 pcs Bandage, first sterile - TYPE III,   1 piece Bandage, first abdominal, sterile  10 pcs Triangular scarf, calico 100 x 100 x 140 cm  10 pcs Set of non-woven compress 7.5 x 7.5 cm 6sl., 2 pcs, sterile 10 pcs Set of non-woven compress 10 x 10 cm, 6 pcs., 2 pcs., Sterile 4 pcs Crepe bandage, cotton 6 cm x 10 m   1. pcs Crepe bandage, cotton 8 cm x 10 m 2 pcs Crepe bandage, cotton 10 cm x 10 m 4 pcs Absorbent gauze 0.8 m2, sterile 2. pcs Surgical patch with absorbent pad 5 x 7 cm, sterile 5 pcs Surgical patch with absorbent pad, 10 x 9 cm, sterile 1 piece Microporous adhesive tape 2.5 cm x 9.1 m   1 piece Scissors with blunt tip  5 pcs Protective film for artificial respiration  1 piece (set) Non-woven patches for small wounds, different in the set, sterile. Dimensions: 19 x 72 mm -5 pcs., 38 x 38 mm - 3 pcs., 25 x 72mm -2 pcs |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | 4 pcs Protective foil gold / silver 10 pcs Safety clips  15 pcs. (1 pkt.) Cleaning wipes, dose a 15 pcs 10 pcs. Latex gloves, size   1. piece Graphite pencil 1 piece Block 2. pcs. PVC waste bag, opaque 1 piece List of contents |  |  |
| **As an example only** | Tosama first aid backpack with equipment Boscarol BOR87400 BPack two rucksacks in one |  |  |
| **Example** | i (2) i (3)  BOR87400 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 45** | **Rescue rope with carabiner hook** | **C** | **D** |
| **Purpose** | Rescuing |  |  |
| **Technical specification** | Requirements:   * Length 30m * Diameter: 11 or 12mm * carabiner hook * carrying bag * standard DIN 14920 or EN 1891 |  |  |
| **As an example only** | RESCUE ROPE, ON F 5260 WITH KARABINER HOOK or |  |  |
| **Example** | Productimage_151030 Productimage_150700 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 46** | **Fire extinguisher** | **C** | **D** |
| **Purpose** | Fire extinguishing |  |  |
| **Technical**  **specification** | 9kg powder, EN3, directive PED 20147/68/EU in MED 96/98/EC. |  |  |
| **As an example only** | Anas PS6-HJ ABC 9KG |  |  |
| **Example** | Slika, ki vsebuje besede besedilo  Opis je samodejno ustvarjen |  |  |

LOGISTIC EQUIPMET

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 47** | **Power generator** | **C** | **D** |
| **Purpose** | Portable power generator 2 kVA inverter |  |  |
| **Technical specification** | Electrical power: 2 kVA Voltage 230V Frequency (Hz): 50 Generator type: Inverter  Size recom: Length (mm)700, Width (mm) 440, Height (mm) 580 Fuel: Gasoline  IP 23  Silnet type |  |  |
| **As an example only** | Eisemann BSKA 2V RSS or Honda 2200i |  |  |
| **Example** | https://eisemann-geko.si/wp-content/uploads/2021/08/BSKA-2V-RSS.jpg |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 48** | **Rubber cable reel** | **C** | **D** |
| **Purpose** |  |  |  |
| **Technical specification** | Cable length: min 40 m Protection: IP68  Cable: minimum quality H07RN-F3G25 Plug type: Schuko (no angles)  Compact and robust lightweight with integrated carrying handle For outdoor use, impact resistant, ageing and weather resistant min 3 earthed sockets with self-closing covers.  EN 61616 |  |  |
| **As an example only** | Friggeri |  |  |
| **Example** | podaljšek-400V |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 49** | **Petrol containers** | **C** | **D** |
| **Purpose** | Plastic fuel can for diesel or gasoline |  |  |
| **Technical specification** | Capacity: 10 litres  Material: Heavy duty plastic Safety requirements UN/BAM  Comes complete with pouring spout |  |  |
| **As an example only** | Oregon OR 042-973, Army Jerry Can Plastic JB-AC10G |  |  |
| **Example** |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 50** | **Pop up folding tent for command post** | **C** | **D** |
| **Purpose** | Rescue operations support |  |  |
| **Technical** | Size: 3x3m |  |  |
| **specification** | Folding type – pop up |  |  |
|  | Material of frame: aluminium |  |  |
|  | Tent (top) material: water repellent, mildew resistant, tear resistant, UV |  |  |
|  | resistant and fire retardant |  |  |
|  | 3 side panels – optional |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **As an example only** | Canopy Folding Tent 3 x 3 pro |  |  |
| **Example** | Immagine che contiene testo, blu  Descrizione generata automaticamente |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 51** | **Camp folding table** | **C** | **D** |
| **Purpose** | Rescue operations support |  |  |
| **Technical specification** | Size app.: 152 x 71 x H74 cm Close size app.: 76 x 71 x H9 cm Weight: app.: 12kg  Load capacity: 100 kg |  |  |
| **As an example only** | Brunner Club 150 |  |  |
| **Example** | Miza Club 150 - Kamp oprema - Camping Orehek |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 52** | **Camp folding chair** | **C** | **D** |
| **Purpose** | Rescue operations support |  |  |
| **Technical specification** | Folding chair with side seat support Weight: app.:  Size: app. 51 x 44 x 48/90 cm Close size: app. 94 x Ø 16cm Load capacity: 110kg |  |  |
| **As an example only** | Brunner Raptor classic |  |  |
| **Example** | Brunner Raptor Classic - Sedie E Brandine | Nencini Sport |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 53** | **Management equipment** | **C** | **D** |
| **Purpose** | Rescue operations support – professional use |  |  |
| **Technical specification** | - 1 GPS MAP: touch screen 6” display, display resolution min. 800 x 480 pixels, rechargeable battery lithium-ion, battery life up to 1 hour, preloaded street maps: Europe |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  | * 1 waterproof digital camera (waterproof 10 m., shockproof 1.5 m.) with GPS, 2 SD memory card 4 GB * 2 plastic boxes with office equipment (approx.. 15 pencils, 15 pens, paper, glue 3 pcs, 1 calculator, 3 scissors, 15 markers & highlighters, 3 rulers, 3 tapes, 2 paper staplers, post-it products 3M 5 pcs, tesa alu tape (2 pcs) * Flags (national) 1\*2 m. * 2 professional binoculars   All equipment is stored in a plastic or alu box |  |  |
| **As an example only** |  |  |  |
| **Example** | office supplies1114 x 753 154 kb jpeg x Images Office Equipment |  |  |

LOTTO 2: FORNITURE DI POLVERE IGNIFUGA PER OPERAZIONI ANTINCENDIO FORESTALI.

**Technical specification**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item 1** | **Fire retardant** | **C** | **D** |
| **Purpose:** | It will be used as a fire retardant in land vehicles for wildfires. |  |  |
| **Technical specification** | pH: 5,5-7,5  Density: 1,25-1,45 g/ml  Colour: Red  Odour: Unique  Appearance: Concentrated Liquid  Water Solubility: Soluble  Flammability: None-flammable  Flash Point: Flameproof |  |  |
| **As an example only** | Neuvatec PW82 |  |  |
| **Example** |  |  |  |
| **Quantity** | 20.000 Kg |  |  |